BusinessPhone Communication Platform 6.0
Commands > Commands 9000...9999

## 9138
Send expensive route warning tone 3

This command defines if the user shall be informed about an alternatively chosen PNR route (e.g. a public route) for the ongoing call setup.

In order to hear the Expensive Route Warning Tone, the command 0187 has to be set for the extensions.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004