BusinessPhone Communication Platform 6.0
Dialogs

## Message and Information System

In this dialog, you can define the settings for the message and information system. To access the dialog, open the “Features” menu in the Configuration directory tree, and then the “Message & Information System” submenu.

#### General Settings

4301 |  | Max time for speech message

4302 |  | Max time for speech info

4303 |  | Max time for speech anno

4304 |  | Time to keep message

4305 |  | Voice message quality

4306 |  | Voice information quality

4307 |  | Voice answer quality

4308 |  | No answer to sender (days)

4309 |  | Keep answered call me

4310 |  | Keep answered voice

4311 |  | Keep answered text

4312 |  | Short message store

4314 |  | Simulate retrieving

4315 |  | Silent detect level VMU-HD

4316 |  | Silent detect time VMU-HD

4317 |  | Play date/time info prior to message

4318 |  | Days to keep archived messages

4319 |  | Days to keep heard messages

#### Predefined Info

4501 |  | Predefined info - Text

4503 |  | Predefined info - Text for cordless

4502 |  | Predefined info - Meaning of digits 1-4

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

See facility description Message System (341/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2004