BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 0F TEXTSTRING

00h TXTINFOQ |  | Ask for text information |
01h TXTINFOACK |  | Answer with text |
02h TXTINFONAK |  | Answer without text |
10h TXTACD |  | Text from ACD |
20h TXTDINAME |  | Name string information (from DI) |
30h TXTGUESTQ |  | Ask for guest check-in data |
31h TXTGUESTACK |  | Answer, with text for guest |
32h TXTGUESTNAK |  | Answer, without text for guest |
40h TXTFSOPI |  | Name string for free seating CTI OPI |
50h TXT3PTYCONF |  | Feature activation request as display text string response |

Revision: F © Ericsson Enterprise 2005