BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1105
Common voice announcement at day

For external incoming calls which are routed to the trunk answering or the rerouting position a voice announcement can be supplied. This command is used to state the day reference number for this voice announcement.

##### Valid data

00-63 |  | See command 4424 Announcements for trunks. The stated reference must have been recorded previously on a system telephone in accordance with command 4424 Announcements for trunks. |
(blank) |  | (no voice announcement) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005