BusinessPhone Communication Platform 7.0
Start of Operation BP Management Suite > What’s new in BMS Version 3 ?

## HTTPS support in the BMS WebServer

Additionally to HTTP (plain text protocol) BusinessPhone Management Suite 3 offers also the encrypted HTTPS.

For a Https connection the following line must exist in the file wwwserver.properties:

- SSLPort = <portnumber> the default well-known SSL-port is 443

Login from Browser:

- https://<servername> if SSL-port is 443
- https://<servername>:<portnumber> if SSL-port is not 443

Error indications from the Browser:

In case that you type: https://NE0008c799b10a you could get:

Press “View Certificate”

#### View Certificate

Select the Tab “Certificate Path”.

#### Certification Path

Press “View Certificate”

#### Certificate - General

Press “Install Certificate”

#### Import Wizard

Press “Next”

#### Certificate Import Wizard_01

Select “Place all certificates in the following store” and press “Browse”

#### Select Certificate Store

Press”OK”

#### Certificate Import Wizard_02

Press “Next”.

#### Certificate Import Wizard_03

Press “Finish”.

#### Root Certificate Store

Press “Yes”.

#### Certificate Import Wizard_04

Press “OK”.

#### Internet Explorer - Internet Options

#### Internet Explorer - Certificates

Error indications from the Browser:

In case that you type: https://NE0008c799b10a you could get:

Press “View Certificate”

- use the name that is stated under Issued to:

https://NE0008c799b10a.sea.ericsson.se

Revision: D © Ericsson Enterprise 2005