BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5426
Create individual mailbox

This directory number is used for the message facility. An extension can set diversion or follow-me to this directory number. In this case all calls to the extension are diverted to the individual mailbox system where the caller can leave a voice message for the extension. If the directory number is called directly, messages for an extension can be retrieved.

Note

Command 5526 Delete individual mailbox number is used to delete the directory number for this facility.
Command 5626 Alter individual mailbox directory number is used to alter the directory number for this facility

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005