BusinessPhone Communication Platform 7.0
System Overview ASB 150 02 Release 15 (BusinessPhone 7.0)

## Operation & Maintenance

### General

Maintenance of ASB 150 02 is possible both locally and remotely. A built-in V.32bis modem on the CPU‑D5/CPU-D5C is used for remote maintenance. The built-in modem is directly connected to the switch and does not occupy an extension position.

### System configuration

All parameters used in the system can be programed via the special operation & maintenance program, BusinessPhone Management Suite. A limited number of parameters can also be programmed from an EXECUTIVE telephone or OPERATOR console.

### BusinessPhone Management Suite (BMS)

BusinessPhone Management Suite is a tool for configuration, administration, upgrading and maintenance of the BusinessPhone system family.

It is self-contained, simple to install and use, and has a very wide range of configuration alternatives: the server software can be installed either at customer or dealer/service centre premises, and can be accessed locally or remotely using a web browser interface. The package supports multiple users and multiple BusinessPhone systems.

The BMS provides a comfortable web browser GUI. No client installation is required as the web browser acts as a client. The BMS is programmed with latest Java technology and is performance optimized for O&M tasks. Servlet technology guarantees fast access with quick web-page build-up in the web browser.

Access to the ASB 150 02 is possible:

- Locally via V.24 interface on BusinessPhone
- Remotely via dial-up (modem on CPU‑D5/CPU‑D5C)
- Remotely via Intranet/Internet by using one of the following connection options:

- Via V.24 Agent which is connected to the LAN
- Direct LAN connection towards the IPU.

- In case of Internet access to a customer site, a firewall permission from the customer may be required.

The BMS can run on any local or networked PC.

The BMS supports multiple configurations:

- Multiple users can access one BMS Server
- One server can maintain and supervise multiple ASB 150 02 systems

### BusinessPhone Extension Assistant (BEA)

BusinessPhone Extension Assistant, is part of of the BMS package targeting the end-users of ASB 150 02. The BusinessPhone Extension Assistant makes an extension configuration quick and simple enough for any Windows user to handle. Functions such as individual abbreviated numbers, diversion settings and assigning function keys can all be carried out from easy-to-follow screen-based windows and menus.

Using BusinessPhone Extension Assistant, users can adapt key system parameters to suit their own particular operational needs.

Revision: C © Ericsson Enterprise 2005