BusinessPhone Communication Platform 7.0
Dialogs

## H.323 Trunk Gateway Data

In this dialog is available for BusinessPhone V6.0 or later.

The IPU hosted H.323 gateway get manually configured the following operational information:

- Own call signalling port number
- Own password which is going to be registered at the gatekeeper as H.323 alias, and will be used for calling system authentication purposes.
- Availability check timer for pre-configured gateways (used in case that there is no gatekeeper)

Additional settings, if the GW is registered at a Gatekeeper

- Own RAS port number
- RAS transport address (i.e. IP address + port number) of the primary gatekeeper position, with which the gateway should register.
- RAS transport address (i.e. IP address + port number) of the backup gatekeeper position, with which the gateway should register whenever the primary gatekeeper position is not reachable. This entry is optional if the primary GK is defined, otherwise prohibited.
- NPI alias aliases the gateway should register with the active gatekeeper - this aliases are going to be registered at the gatekeeper as public or private party numbers.

Registration Information:

- Registered with primary gatekeeper
- Registered with backup gatekeeper
- Can't read registration information
- Not registered – Not configured
- Not registered - Near end network out of order
- Not registered - No response from gatekeeper
- Not registered - gatekeeper refused registration

For more information about a setting or a field, click on the command link in brackets to open the online help system. See also System Description (1551-ASB 150 02 Uen).

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

### Other IPU Board Data dialogs

On top of the dialog, you find a navigation bar that provides access to the following IPU Board Data dialogs:

- Basic Data

- To go to the Basic IPU Data dialog.

- Ports

- To go to the Port configuration data dialog.

- Gatekeeper

- To open the Gatekeeper Data dialog.

- H.323 extension gateway data

- To go to the H.323 Extension Gateway Data dialog.

- H.323 trunk gateway data

- The dialog you view right now.

- Licensing

- To go to the Voice Channel Licensing dialog.

- Board Configuration

- To open the Board Configuration dialog.

Revision: B © Ericsson Enterprise 2005