BusinessPhone Communication Platform 7.0
Dialogs

## Call Information Logging

You can define what kind of information should be recorded in the call information log.

To access the dialog, open the “Features” menu in the Configuration directory tree and click on “Call Information Logging”.

The following options are available:

6201 |  | Log internal calls?

Check this box if you want to log all internal calls.

6202 |  | Log incoming calls?

Check this box if you want to log all incoming calls.

6203 |  | Block log output?

Check this box, if you want to block the log output temporarily, for example in case of a paper jam or during maintenance of the system.

6204 |  | Digits to log

Select “dialled” if you want to record all dialled digits; select “sent” if you want to keep a record of all sent digits.

6205 |  | Bar outgoing calls for guest

Check this box if no outgoing calls should be possible while using a guest extension.

Note

For more information about a field or a setting, click on the command link in brackets.

#### Actions

Submit |  | To send the settings to the system. |
Reload |  | To load the current system settings and to discard all entered data or changes. |

For more information, see facility description Call Information Logging (CIL) Function (140/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005