BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1954
Charging information provided to the TE?

This command states whether or not charging information is provided by the terminals on the interface. The type of charging AOC (Advice Of Charge) is defined by T-interface parameters. If it is not provided, the charging information will not be sent to the terminal.

##### Valid data

Yes |  | AOC is not provided |
No |  | AOC is provided |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005