BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0148
Automatic display of metering info?

Enable/disable automatic display of metering information.

During EXTERNAL calls it is possible to display different types of metering information such as ”Money”, “Pulses”, “Duration” etc. The type of information to be displayed is selected with command 0147 Type of meter info. Command 0148 Automatic display of metering info? defines the default state for displaying information when a new outgoing call is initiated.

Two states are possible:

Automatically:

When a new external call is initiated/answered, the display is automatically and repeatedly updated with the type of metering information selected by command 0147 Type of meter info.

Not automatically:

When a new external call is initiated/answered, the display is NOT updated automatically with metering information.

Irrespective of state, the cost information can be enabled/disabled with help of a menu key. The menu key has a toggle function and can be pressed several times during a call. The temporary selection is kept during the current call but when the next call is initiated, the default state selected with command 0148 Automatic display of metering info? will override the temporary selection.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005