BusinessPhone Communication Platform 7.0
Start of Operation BP Management Suite

## BMS execution

During the installation procedure, the whole BMS SW package is installed on a directory on your PC. If you have not changed the names, it is stored in directory C:\Program Files\Ericsson\BMS\Server.

To start the BMS click on the BMS Server shortcut on the desktop or in the Windows start menu.

The BMS server and the WEB server will be started and the following two dialogs will pop up on the screen:

- BMS server screen
- Web server screen

As long as the BMS server is up and running, these two dialogs have to exist. The BMS server screen shows the status of the BMS server. The Web server screen will show the status of the Web server.

The BMS server and the BMS Remote v.24 Agent do not run on the same PC at the same time. The BMS Remote v.24 Agent is designed for remote connection of the BusinessPhone via V.24 and/or modem on the LAN to the BMS. For a single installation of the BMS the BMS Remote v.24 Agent is not required. The direct connection types (direct serial, direct modem) can be used.

### BMS Server Screen

This dialog shows whether the BMS server is started correctly. In the display area of the screen the status of each SW block of the BMS is displayed.

If one of the entries in the screen shows an error, the server will not be start correctly. Handling by means of the BMS will cause errors.

### Web Server Screen

This dialog shows whether the Web server has been started correctly. In the display area of the screen the settings and the status of the web server will be displayed.

If there are reasons for changing parameters for the Web server, e.g. change the port, the server has to be stopped. Thereafter the different fields can be changed.

##### The different fields are

- Use Config File
- Use settings

#### Use Config File

There is a default file which contains the default settings of the WEB server.

The default settings are defined as follows:

RootDir =
C:\Program Files\Ericsson\BMS\Server\wwwroot
Port = 80
DefaultFile = default.htm
LogDir =
C:\Program Files\Ericsson\BMS\Server\wwwlog
ServletPath =
C:\Program Files\Ericsson\BMS\Server
ServletProperties = C:\Program Files
\Ericsson\BMS\Server\servlet.properties
ServerName = < hostname >

#### Use settings

- Port

- This is the port where the Web server will run when it is started.

- Web Root Directory

- This is the Web server root directory which contains the necessary files for running a WEB server-

- Default File

- The default file that will be called upon browser login in the BMS server.

- Log Dir

- This is the directory where the log files will be stored.

- Servlet properties

- This is the Servlet property file for the WEB server.

Note

If one of the settings is changed, make sure that the data that are required for a WEB server are correct, e.g. files in the directories, data in the files, file names etc.

If the default port number 80 is changed to another number, the number must be entered in the address in the browser, otherwise the browser cannot access the BMS server.

<name of the PC>.<network address>:<port number>

e.g.: localhost

Revision: D © Ericsson Enterprise 2005