BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3710
Pause time

If the active agent is in pause state he or she will be logged out automatically if that time elapses. The timeout for the pause state is defined in minutes. The time will be retriggered when the agent gets into idle state. i.e has no ongoing task. The time will be stopped when the agent gets out of the idle state.

Valid data

1-30 |  | minutes |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005