BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5512
Delete answer number for meet-me

ASB 150 permits connection of external equipment for paging via radio or a magnetic loop. Connection takes place via a trunk (external line) board that has been reserved for this purpose.

This command is used to delete the call number for “meet-me” paging.

Meet-me paging means that the pagee answers by dialling the directory number that can be deleted with this command, followed by his/her own number.

Commands 5510 Delete call number for standard paging and 5511 Delete call number for alternative paging are used to delete other directory numbers (if any) that have been created for paging.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005