BusinessPhone Communication Platform 7.0
Dialogs

## ASB 150 02 licensing

### License Status

The license status table provides read only information for following values:

- Licensing board
  States the board position which carries the license file
- Remaining trial time
  States the remaining operating hours for all features which have no valid entry in the license file. The counter will be decreased in 5 minutes steps.
- System ID
  States either the serial number of the connected FECU or the serial number the CPU-D5/CPU-D5C. If a CPU-D5/CPU-D5C is installed in the system with a connected FECU, then always the FECU serial number will be used as the system ID.

Note

The FECU serial number contains the dedicated software release as well as the FECU Index. The first digit on the left site describes the software release (0=R9/R10, 1=R11, 2=R12, 3=R13). The second digit on the left site describes the FECU-Index (1=Index 1, 2 =Index 2, ......A=Index10). According to the example above a FECU from R13 Index 10 is used.

- Serial Number of Flash Disk
  States the unique serial number of the storage media on which the license file is stored.
- LZY Information
  States article number and revision of the CSW

### ’Licensed feature’ table

The table provides an overview of all features which are requiring a license:

- License Name
  States all the features (feature packages) which require a license entry.
- License value
  States the licensed number of the user or the feature level of the licensed feature. An additional parameter displayed in brackets, is a typical indication for a not licensed feature.

- (Trial)
  indicates that the feature is only available until the trial time expires.
- (Basic)
  indicates that the feature is limited to the feature level which defined by the Basic license.
- (FECU)
  indicates that the feature is limited to the feature level which defined by the connected FECU.
- (System enabled)
  indicates that the feature has been enabled due a certain combination of CSW, Basic license and installed HW.

#### Values in the ’Licensed feature’ table versus parameters in the license file:

Indication in the BMS |  | Indication in the license file | Comment
License Name | License value | Description | License entry | License value
Basic | No | Enabled (Yes/No) | - | - | after trial period if no appropriate license entry exists in the license file
Yes (Trial) | - | - | during trial period
Yes | BASIC_LICENSE | 1 | always available on CPU-D5/CPU-D5C boards
Mobile Extension | 0 | Users | - | - |
100 (Trial) | - | - | during trial period
2 (Basic) | - | - | defined by Basic license
5-100 | MOBILE_EXT_LICENSE | 5 -100 |
Unified Messaging | 0 | Users | - | - |
200 (Trial) | - | - | during trial period
2 (Basic) | - | - | defined by Basic license
20-200 | UNIFIED_MSG_LICENSE | 20 -200 |
CTI | 0 | Users | - | - | after trial period, if neither an appropriate entry in the license file nor an appropriate FECU is installed
80 (System enabled) | - | - | if CSW Release 15 R3A or higher and a Basic license entry exists in the license file; CTI license 80 is not installed
80 (Trial) ***) | - | - | during trial period
2 (Basic) **) | - | - | defined by Basic license
80 (FECU) | - | - | defined by connected FECU Index 6-10 - after trial period and no appropriate license file
7 **) | CTI_LICENSE | 7 | defined by appropriate CTI license entry
80 | CTI_LICENSE | 80 | defined by appropriate CTI license entry
Networking | Not enabled/0 | Feature level/Trunks | - | - | after trial period, if neither an appropriate entry in the license file nor a FECU is installed
| Full/Unlimited (Trial) | - | - | Full digital networking with unlimited trunk interfaces (during trial period)
| Full/2 (Basic) | - | - | Full digital networking with 2 trunk interfaces (defined by Basic license)
| Full/2 (FECU) | - | - | Full digital networking with 2 trunk interfaces (defined by FECU Index 1)
| Full/4 (FECU) | - | - | Full digital networking with 4 trunk interfaces (defined by FECU Index 6)
| Standard/32 (FECU) | - | - | Standard digital networking with 32 trunk interfaces (defined by FECU Index 2, 7)
| Standard/unlimted (FECU) | - | - | Standard digital networking with unlimited trunk interfaces (defined by FECU Index 3, 8)
| Full/32 (FECU) | - | - | Full digital networking with 32 trunk interfaces (defined by FECU Index 4, 9)
| Full/Unlimted (FECU) | - | - | Full digital networking with unlimited trunk interfaces (defined by FECU Index 5, 10)
| Standard/unlimited | NETWORKING | 3 | Standard digital networking with unlimited trunk interfaces
| Full/32 | NETWORKING | 4 | Full digital networking with 32 trunk interfaces
| Full/Unlimted | NETWORKING | 5 | Full digital networking with unlimited trunk interfaces
| Standard/unlimited (System enabled) | - | - | Standard digital networking with unlimited trunk interfaces (if CSW Release 15 R3A or higher, a Basic license entry in the license file exists and an IPU board is installed and the trial time is expired)
VOIP Gateway | No | Enabled (Yes/No) | - | - |
Yes | VOIP_GATEWAY | 1 |
CPU-D5C *) | 3 | Maximum boards | - | - |
Unlimited | MAX_BOARDS | 63 |
BackStage | 0 | Users | - | - |
80 (Trial) | - | - | during trial time
2 (Basic) | - | - | defined by Basic license
7-80 | EXT_APP BACKSTAGE | 7-80 |
BEA | 0 | Users | - | - |
250 (Trial) | - | - | during trial time
10 (Basic) | - | - | defined by Basic license
50-250 | EXT_APP BEA | 10-250 |
CCA | 0 | Users | - | - |
40 (Trial) |  | - | during trial time
2 (Basic) |  | - | defined by Basic license
5-40 | EXT_APP CCA | 5-40 |

*) Only displayed in conjunction with a CPU-D5C in order to upgrade the board to a CPU‑D5 to get no limitation in the number of supported board positions.

**) Only displayed if the installed CSW is older than Release 15 R3A

***) Displayed during trial time if the installed CSW is older than Release 15 R3A or CSW is Release 15 R3A or higher and no Basic license exists.

#### Actions:

- Export license file
  This button is used to fetch the license file from the board on which it is stored and to export it to a desired destination on the PC or LAN. For further details see To export the license file.
- Import license file
  This button is used to import a license file, which was received from the Ericsson License Center, into the system to replace the existing one. For further details see To import the license file
- Show license file
  This button is used to view the content of the license file. For further details see Show license file.
- Reload
  This button is used to refresh all indications from the license dialog.

For further details please refer to: ASB 150 02 Software key based licensing

Revision: B © Ericsson Enterprise 2005