BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0152
Override LCR?

The command defines whether or not the extension is permitted to override the least cost routing flag for the trunk.

If this flag is true for the extension, the call will proceed without LCR control and TCD category as for a normal external call. In this situation the TR block will not make any reroute to LR. The call will proceed as without LCR.

##### Valid data

Ýes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1 |  |

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005