BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1803
Irrelevant digits at automatic incoming traffic

The command is used to state how many initial digits in the incoming number shall be omitted before the number is analyzed.

Value = 0-3

Initial value: not in use

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005