BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1948
CLIR Override at incoming calls

This command states if the CLIR (Calling line identification restriction) shall be overridden and a received Calling number shall be presented. This number will be used for display and other (CIL, MIS, CTI) purposes.

Note

This feature is intended for usage at emergency numbers. Before enabling ‘CLIR Override’ it has to be checked, if the presentation of restricted numbers is supported by the public net and subscribed.

##### Valid data

Yes |  |  |
No |  | (default) |

This command is valid for ISDN T- and Q-interface

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005