BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xAD
Battery Backed Up RAM Check Failed

Default definition: |  | ALARM |
Used by block: |  | OS |
Category: |  | DESIGNER |

This warning is generated by ARRAY.CHECK, if an incorrect array was found.

- D1: Statusbyte
- D2: Number of records with checksum errors

- FFh: Indicates 255 or more checksum errors found

- D3: Array identity, high byte
- D4: Array identity, low byte

Revision: K © Ericsson Enterprise 2005