BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5614
Alter group call pickup no.

With this command it is possible to change (alter) the directory number for the call pickup ext. group facility.

If you want to change to a number that is in conflict with the old number, this cannot be achieved directly. In this case first change to any free number, and then change the latter to the desired number.

However, references to previously valid numbers will remain. These references should be removed or replaced by the new number. See description of command group 56 listing commands referring to directory numbers.

If no number is stated, the call number will be cancelled.

A new call number can be created with the same command.

To delete the call pickup code, see command 5505 Delete group call pick up code.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005