BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x61
Trunk Line Error

Default definition: |  | ERROR |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

The line to the connected exchange has a faulty/no polarity (line guard).

- D1: Card position
- D2: Individual number
- D3: Undefined
- D4: Undefined

#### Recommended action

Check the line polarity on the trunk(s).

Revision: K © Ericsson Enterprise 2005