BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1410
Time for recall on camp-on

On inquiry to a busy extension it is possible to camp-on the parked call, i.e. effect transfer on busy. The command is used to determine the recall time on transfer to a busy extension, i.e. if the party requested does not go free or answers within the stipulated time, recall will be activated.

Value 0-255 seconds

For camp on of trunks see command 1008 Camp-on to answering position?.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005