BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5408
Create voice answer

The voice answer (recorded announcement) facility can be included in ASB 150. Voice answer means that the PABX can automatically supply a recorded announcement in reply to incoming calls for those directory numbers which have been defined for this facility.

With this command it is possible to create an answering position with automatic voice answer that has the stated directory number. The answer positions with automatic voice answer can be assigned any number that is free and does not conflict with existing directory numbers. See command group 56.

ASB 150 permits a maximum of 16 answering positions with automatic voice answer.

A system telephone set up for system programming is to be used for recording voice answers (recorded announcements). Command 4701 Reference number for voice answer states which recorded voice answer shall apply for each answering position with automatic voice answer.

See also commands 4701 Reference number for voice answer and 4702 Voice answer storage.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005