BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## B2 SERVICE

0 SENAK |  | Requested service is not implemented |
1 SEMCIDREQ |  | MCID request |
2 SEMCIDACK |  | MCID accepted |
3 SEMCIDNAK |  | MCID rejected |
4 SEMLTREQ |  | ISDN call waiting request |
5 SEMLTACK |  | ISDN call waiting request: accepted |
6 SEMLTNAK |  | ISDN call waiting request: rejected |
7 SEAOCERES |  | AOC-E charging information (CFPR impact) |
8 SEROUTEDAT |  | ROUTE own location code |
9 SERTIME |  | AutoTimeSync request |
10 SERTIMEANSW |  | AutoTimeSync answer containing date/time |

Revision: F © Ericsson Enterprise 2005