BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8109
Paging meet-me time

For meet-me paging the pagee can answer by dialling an answer code followed by his/her own directory number.

This command is used to determine the time for a pagee to answer a meet-me paging call.

Range of values: 10-255 s

If no answer is received during the stipulated time, the paging call will be cleared down.

If the pagee does not answer an extended external call and the extending party is to be recalled, the time value in this command shall be higher than that in command 1409 Time for recall on transfer before answer.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005