BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3023
Day/night trunk group 1

This command is used to state which A-categories are permitted to alter the function for day/night switching with respect to trunk group 1. The procedure for day/night switching = *81#

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005