BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5412
Create answer number for meet-me

ASB 150 permits connection of external equipment for paging via radio or a magnetic loop. Connection is achieved via a trunk (external line) board that has been reserved for this purpose.

This command is used to create a function for answer in accordance with the meet-me principle. Meet-me paging means that the pagee answers by dialling the directory number that has been defined by this command followed by his/her own number. The stated directory number must be free and must not conflict with any existing directory number.

Commands 5410 Create call number for standard paging and 5411 Create call number for alternative paging are used to create functions for setting up different types of paging.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005