BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x8D
TAU Parameters Missing

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | EX |
Category: |  | MAINTENANCE |

The extension has been programmed as a data extension, but the record for TAU parameters has not been created. This error can be corrected by reprogramming.

- D1: Card position for the extension
- D2: Individual number for the extension.
- D3: Undefined
- D4: Undefined

#### Recommended action:

First, program the extension as a non-data extension and then program it as a data extension again.

Revision: K © Ericsson Enterprise 2005