BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3024
Day/night trunk group 2

This command is used to state which A-categories are permitted to alter the function for day/night switching with respect to trunk group 2. The procedure for day/night switching = *82#

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005