BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4805
Member of loudspeaker paging group 4 ?

These commands are used to state which extensions in the respective group are to be called in conjunction with paging in the respective group and to define the individual volume for loudspeaker paging calls.

To be able to start or answer a loudspeaker paging call an extension shall have a programmable key.

To be able to initiate a call the extension must also have a facility (service) category that is open for loudspeaker paging calls.

Commands in this group (48) require that the relevant loudspeaker paging group has been initiated, which takes place the first time the command for categorisation of the loudspeaker paging group is issued.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005