BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4323
Number of OCN repetitions

This command determines how many attempts (1-10) take place until the notification is cancelled.

If a notification is unsuccessfull, the system will redial again as long as the number is not reached. The counting starts from zero, which means that one more notification will be performed than the value of this command.

The appropriate time table which is described in the 4320 Notification scheduling profile, shows you the maximum attempts in dependance of any selected profile.

Revision: E © Ericsson Enterprise 2005