BusinessPhone Communication Platform 7.0
Dialogs

## Fictive Number - Modify Series

In this dialog, you can modify a series without risking the loss of any data.

To access the dialog, open the “Number series” menu in the Configuration directory tree and click on “Fictive”. Now click on a “Modify Series” link of a number series. Alternatively, select the “Modify Series” option from the context menu of a number series.

If a new number series covers the same range as the old series, all data will be copied. If the old series is part of the new series, the data is moved to the corresponding position in the new series.

If none of the above conditions apply, the data from the old series is copied to the beginning of the new series, including all available data. If the new series is shorter than the old one, a part of the data will be ignored.

For further information, about a field, click on the command link in brackets. See also section Fictive Number Series and facility descriptions Fictive Number (201/15534-ASB 150 02 Uen) and Abbreviated Number dialing - common numbers (101/15534-ASB 150 02 Uen).

### To modify a number series

- Enter the new number series in the “Change to” field.
- Click on the Submit button. The dialog refreshes, now showing the altered number series in the dialog and in the Configuration directory tree.

Note

If the entered number series causes a conflict with any directory number or setting, an error message is displayed.

#### Actions

Submit |  | To send the changes or settings to the system. |

Revision: B © Ericsson Enterprise 2005