BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8604
Guest extension message when retrieving

When a guest extension calls the individual mailbox system directly by pressing the msg-key or dialling *59#, a retrieving session of individual messages is started. The caller is then greeted with a welcome announcement. In this command the voice reference for the announcement is stated. It is possible to state one announcement for each language code. The guest will be greeted with the language code given by check in.

The reference is supposed to have been recorded according to command 4416 Retrieving individual. Note that recording according to command 4416 is only possible on a VMU-HD board.

To state a language code see commands 8009 Wake-up language 1-8011 Wake-up language 3.

##### Valid data

0-15 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005