BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8507
Common mailbox welcome 1

In this command the reference number for the welcome message upon diversion of the caller to a common mailbox can be programmed. If the diverted party is a hotel extension, the welcome announcement is played in the language the guest is checked in with. The welcome announcement stated in command 8507 Common mailbox welcome 1 is played for a guest extension with language1 or if the language is unknown. In command 8508 Common mailbox welcome 2 and 8509 Common mailbox welcome 3 welcome announcements for language 2 and language 3, respectively, are stated.

To program a language code see commands 8009 Wake-up language 1-8011 Wake-up language 3.

The given reference is supposed to have been recorded according to command 4417 Welcome common. Note that recording acc. to command 4417 is only possible on a VMU-HD board.

##### Valid data

0-15 |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005