BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2185
H.323 Extension GW Q.931-port

Defines the Q.931‑port of the H.323 Extension Gateway. The H.323 Extension GW Q.931‑port must not confilct with any other Q.931port.

If modified, a restart of the IPU is required.

##### Valid data

0-65535 |
1720 (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005