BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2272
Trunks Available for Automatic Redial

This command defines the number of trunks which are placed at automatic redial disposal (means that a number of automatic redial attempts can be executed at the same time).

The parameter is used to limit the system resources.

##### Valid data

Valid values: |  | 1 - 8 |
Initial values (default): |  | 2 |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005