BusinessPhone Communication Platform 7.0
Dialogs

## Digital Link Parameters

You can define how long a link will take to recover after an alarm had been activated. This duration is called the consolidation time. The default value is 10 seconds. Furthermore, the dialog allows you to set the link priority for synchronization between digital connected systems.

The following options are available:

2060 |  | Consolidation time from alarm to OK

2061 |  | First priority link for synchronisation

2062 |  | Second priority link for synchronisation

2063 |  | Third priority link for synchronisation

2064 |  | Fourth priority link for synchronisation

2065 |  | Fifth priority link for synchronisation

To access the dialog, open the “System” menu in the Configuration directory tree. Then open the “System parameters” submenu and click on “Digital link parameters”.

For more information about a field or a setting, click on the command link in brackets. See also facility description Networking – Based On Digital Lines (365/15534-ASB 150 02 Uen).

#### Actions

Submit |  | To set the changed parameters. |
Reload |  | To reload the current parameters. |

Revision: B © Ericsson Enterprise 2005