BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## D0 IPDATA

01h IPBASWR |  | RP Write basic IP data record |
02h IPRECWR |  | RP Write extended IP data record (linked record) |
03h IPWRACK |  | RP Positive write acknowledgment |
04h IPWRNAK |  | RP Negative write acknowledgment |
05h IPRDREQ |  | RP Request for read of dynamic data |
06h IPRDANSW |  | RP Answer to read request for dynamic data |
07h IPDATARDY |  | RP Write IP data ready |
08h IPEXREGPAR |  | RP Write extension registration parameter |

Revision: F © Ericsson Enterprise 2005