BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2114
Valid Account Codes

This command is used to state account codes which will be used as reference for validity check of all user entered account codes during traffic. Only account codes specified by this command are accepted as valid account codes

Account codes are 1 to 10 digits long numbers used to control access to external lines. Valid digits are 0 to 9.

This command offers in BMS to enter a list of ACC codes. BMS supports adding, deleting and altering of ACC codes.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005