BusinessPhone Communication Platform 7.0
Dialogs

## H.323 Trunk Gateway Control

This dialog shows Peer H.323 trunk GW status information as experienced by every single IPU board in the system (even by pure Extension IPUs). The peer H.323 trunk GWs are identified by its Node reference and the pre configured Network IP-Address. The IPU boards are represented by its card position in the system. The following table describes meaning of the reported status information:

Value | meaning | possible reason
? | Supervision status Unknown | signaling protocol =101
NOK | Not reachable Supervision mechanism active | LAN error peer GW is out of order the own IPU is disconnected from the LAN
OK | Reachable everything OK and traffic is enabled |

#### Actions

Reload |  | BusinessPhone tries to reach the peer H.323 trunk GWs and updates the status; BMS fetches the updated status |
Network IP address |  | To return to the previous window. |

Revision: B © Ericsson Enterprise 2005