BusinessPhone Communication Platform 7.0
Start of Operation BP Management Suite

## BEA Licenses

### Generating a request

Initially, any given installation of the BusinessPhone-Management Suite (BMS) does not contain BEA, the BusinessPhone Extension Assistant.

Note

Since ASB 150 02 Release 15 the basic licence of ASB 150 02 includes 10 BEA users.

It is possible to automatically obtain one Test Account for BEA-Usage called “beademo”.

If an order for BEA-Licenses is placed, you must send the BEA-License-Request to Ericsson, too.

### Programmable functions

- 03xx Programmable keys
- 04xx Individual Abbreviated Numbers
- 0112 Outgoing fixed diversion
- 0172 Destination for internal calls
- 0173 Destination for external calls
- 0156 Direct diversion
- 0157 Diversion on no reply
- 0158 Diversion on busy
- 0159 Direct diversion
- 0113 Outgoing individual diversion
- 0147 Type of metering info1
- 0148 Automatic display of metering info
- 0165 Diversion on no reply to slave
- 0166 Slave always logged on
- 0167 Ring on master and slave

#### Additional information

- Internal directory book (entries that are marked as invisible in the directory book are not displayed)
- External directory book
- Assignments of own extension

- Member of PBX group nn (3401)
- Member of Call Pickup group nn (4201)
- Member of Voice Paging group nn (480n)
- Member of ACD group nn

### After connection

After successful connecting to the exchange, the following information is retrieved:

1. Type of telephone as received from the system. This will be used to determine the correct picture for the GUI.
2. COS (Class of Service) assigned to the extension. This value determines the functions that may be assigned to a programmable key. Restricted functions are not offered to be (re)programmed.

### Creating an account for testing BEA

If no BEA-License is installed on the system you can create a “beademo” user account.

- Selecting

- Licensing

- Order BEA-Demo-License, by clicking “YES”

Answering this question with “Yes” will create an user called beademo, which needs to be configured using the System Administration Tool since valid ASB- and Extension-Entries are needed.

- When you are logged on, select the Security Menu, and then User List and modify the user “beademo”

- Select system and define extensions

### BEA up to ASB 150 02 Release 14

#### Creating a BEA-License-Request

- Selecting

- Licensing

- Order Bea License, by clicking “NO”

- Create a BEA-Order Request

- Define the number of Licenses

The Primary Request offers a range of licenses (50, 100, 150, 250) for selection. After selecting the appropriate amount (contact your Ericsson representative for pricing information) just clicking on “Done” is necessary. To order the creates request-file (“bea_lic.req”) which is placed in the ../BMS/Server directory of the installation has to be sent to Ericsson.

#### Upgrade Request

If there are already BEA-licenses installed, neither will there be an offer to create a demonstrational bea-user nor will the Primary List be shown. Instead an Upgrade-List is displayed offering only such possibilities as might be possible to install without creating more than 250 licenses.

#### Installing the BEA-License received from Ericsson

After the order has been processed the customer will receive an electronic license-key to unlock the feature order. This key should be contained in a file named bea.prm. If by any change the license file is named differently it is of paramount importance to rename it to the required name “bea.prm”.

After the import of BEA license was successful, restart customer BMS server.

### BEA since ASB 150 02 Release 15

Since ASB 150 02 Release 15 BEA licenses are handled as any other external application (BackStage, CCA); see Maintenance instructions (1541‑ASB 150 02) Licensing

### Check if temporary master profile

If the 7th position is a “F”, than it is a temporary master

Revision: D © Ericsson Enterprise 2005