BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1935
Pre-digit removal for private plan with local type of number

This command specifies the number of pre-digits to be removed to get the internal number for “called party” at an incoming ISDN-call using number plan private, and the number type is LOCAL.

Value: 00-15

Minimum required authority level from telephone:

Accessible via BMS:

Revision: F © Ericsson Enterprise 2005