BusinessPhone Communication Platform 7.0
Dialogs

## IPU Licensing

The number of the supported bi-directional Voice-over-IP channels on the IPU is defined by a license file on the Compact Flash card.

The name of the license file as well as the number of the different licenses depend on the release of the central software.

Release | File name | Application image (Firmware) RYS 102 541/1 | Number of licensed voice channels
12 | IPU.ULK | < R2A | 4, 8
LICCFG.ULK | ³ R2A | 4, 8
³ 13 | LICCFG.ULK | ³ R2A | 4, 8, 16

#### ASB 150 02 R12

The license file is only available in conjunction with a Compact Flash card. In case of license upgrades, the Compact Flash card has to be replaced by a Flash card with a higher license.

Article number of the license | Function
LZYBS 203 13/4 | 4 voice channels
LZYBS 203 13/8 | 8 voice channels

Note

The license file is linked to the unique serial number of the Compact Flash card and therefore does not work on any other Compact Flash card.

#### ASB 150 02 R13

Compared to ASB 150 02 R12 two different kind of licenses exist:

- a temporary license for 28 days
- a final license.

For more information about IPU licensing, please refer to section Voice Channel Licensing and to the Maintenance Instruction(1541-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005