BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1957
Number restriction allowed from TEs?

This command states whether the terminal user(s) are allowed to restrict the presentation of the own calling/connected party number in the network.

##### Valid data

No |  | restriction not allowed |
Yes |  | restriction allowed |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005