BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6511
Listing of data for common short numbers

A printout of the programmed dataposts is done. The assignment of a namestring to a common short number is done by using the command 5413 Create common abbreviated number series.

Command 6011 Autoselect allowed? of the connected printer must be set to YES.

Value |
ALL | Dataposts for all common short numbers are printed.

Minimum required authority level from telephone: 1

Accessible via BMS: No

Revision: E © Ericsson Enterprise 2005