BusinessPhone Communication Platform 7.0
Start of Operation BP Management Suite

## BMS Remote v.24 Agent execution

During the installation procedure the whole BMS Remote v.24 Agent SW package is installed on a directory on your PC. If you have not changed the names, it is stored in directory C:\Program Files\Ericsson\BMS\RemoteAgent.

Note

The BMS Remote v.24 Agent is not needed for direct connetction to a BusinessPhone IPU_ board.

To start click on the BMS Remote v.24 Agent shortcut on the desktop or in the Windows start menu.

##### The fields in the screen have the following meaning

- Connected server: shows the server that is connected to the BMS Remote v.24 Agent via the LAN network. As long as there is no address displayed on the screen, the BMS Remote v.24 Agent waits for BMS server connection.
- My IP Address: shows the IP address of the PC on which the BMS Remote v.24 Agent is installed.
- My Port: shows the port on which the BMS Remote v.24 Agent will communicate with the BMS server.
- My Host Name: shows the host name of the PC on which the BMS Remote v.24 Agent is installed.

The buttons at the bottom of the screen have the following meaning:

- Trace On: A click on this button will start the trace, which displays the messages that are sent and received from the BusinessPhone. The button is changed to Trace Off. To stop the trace click on Trace Off. The trace needs resources of the PC. Therefore it should be stopped if it is not needed.
- Start: The BMS Remote v.24 Agent will be started on a specific port. The default port number is 7777. If this port is occupied by another process and the BMS Remote v.24 Agent cannot be started on this port, the dialog will be changed:

- It is now possible to change the number of the board in the field My Port and start the BMS Remote v.24 Agent again by clicking the button Start.

- Exit: A click on this button will stop the BMS Remote v.24 Agent and close the application. The user will be prompted by a message box:

The information displayed in the fields My IP Address, My Host Name and My Port has to be used in the settings of the connection parameter for the desired BusinessPhone.

Revision: D © Ericsson Enterprise 2005