BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1409
Time for recall on transfer before answer

The command is used to determine the recall time on transfer before answer, i.e. recall takes place if the party to whom transfer is attempted does not answer within the stipulated time.

Value 0-255 seconds

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005