BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6803
Tenant-Route

This command is used to define a route directory number for outgoing calls used by a given tenant group.

##### Valid data

digits | remark
empty | default for tenant group 0‑15 (up to R13)
empty | default for tenant group 1‑15 (since R14)
0-4 | 0 ‑ 9, *, #
0 | default for tenant group 0 (since R14)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005