BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2104
Recall on individual parking

For individual parking from system DIALOG 2753 or DIALOG 2754 an extension user who has parked a call will be recalled after a predetermined time if he/she has not used his/her telephone actively in the meantime. (Extensions with R-button will always be recalled immediately after an unsuccessful inquiry call is terminated).

This command determines when (after what time) the recall shall take place:

0 = Diversion will never take place |  |

1-255 = Diversion time in seconds |  |

External calls will be diverted to the diversion position for the trunk unless the extension that parked the call does not answer the recall within a predetermined time. This time is determined by command 1406 Wait time before ring back/rerouting at not answered calls.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005