BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0108
Camp-on allowed?

On an inquiry to a busy extension it is possible to camp-on the parked call, i.e. transfer towards busy. On a call to a busy extension it is also possible to camp-on.

The command states whether the extension permits other extensions to camp on and to use callback to the extension.

The PBX-operator can always place a call on camp-on and initiate call waiting.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005